Filetype: IR signals file
Version: 1
# 
# ViewSonic Remote Control A-00010219
# 
name: POWER
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0C 00 00 00
# 
name: MUTE
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0D 00 00 00
# 
name: SLEEP
type: parsed
protocol: RC5
address: 00 00 00 00
command: 26 00 00 00
# 
name: DISPLAY
type: parsed
protocol: RC5
address: 00 00 00 00
command: 12 00 00 00
# 
name: P.MODE
type: parsed
protocol: RC5
address: 00 00 00 00
command: 1A 00 00 00
# 
name: S.MODE
type: parsed
protocol: RC5
address: 00 00 00 00
command: 24 00 00 00
# 
name: 1
type: parsed
protocol: RC5
address: 00 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: RC5
address: 00 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: RC5
address: 00 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: RC5
address: 00 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: RC5
address: 00 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: RC5
address: 00 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: RC5
address: 00 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: RC5
address: 00 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: RC5
address: 00 00 00 00
command: 09 00 00 00
# 
name: ALT+TAB
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0B 00 00 00
# 
name: 0
type: parsed
protocol: RC5
address: 00 00 00 00
command: 00 00 00 00
# 
name: ALT+F4
type: parsed
protocol: RC5
address: 00 00 00 00
command: 22 00 00 00
# 
name: INPUT
type: parsed
protocol: RC5
address: 00 00 00 00
command: 28 00 00 00
# 
name: ASPECT
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 3E 00 00 00
# 
name: MENU
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2E 00 00 00
# 
name: ALT
type: parsed
protocol: RC5
address: 00 00 00 00
command: 32 00 00 00
# 
name: TAB
type: parsed
protocol: RC5
address: 00 00 00 00
command: 33 00 00 00
# 
name: DESKTOP
type: parsed
protocol: RC5
address: 00 00 00 00
command: 34 00 00 00
# 
name: X
type: parsed
protocol: RC5
address: 00 00 00 00
command: 35 00 00 00
# 
name: D.MENU
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2D 00 00 00
# 
name: D.TITLE
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2F 00 00 00
# 
name: UP_ARROW
type: parsed
protocol: RC5
address: 00 00 00 00
command: 1C 00 00 00
# 
name: LEFT_ARROW
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2C 00 00 00
# 
name: RIGHT_ARROW
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2B 00 00 00
# 
name: DOWN_ARROW
type: parsed
protocol: RC5
address: 00 00 00 00
command: 1D 00 00 00
# 
name: ENTER
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0A 00 00 00
# 
name: D.USB
type: parsed
protocol: RC5
address: 00 00 00 00
command: 30 00 00 00
# 
name: D.SETUP
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0F 00 00 00
# 
name: CH_NEXT
type: parsed
protocol: RC5
address: 00 00 00 00
command: 20 00 00 00
# 
name: CH_PREV
type: parsed
protocol: RC5
address: 00 00 00 00
command: 21 00 00 00
# 
name: EPG
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 38 00 00 00
# 
name: FAV
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 39 00 00 00
# 
name: VOL+
type: parsed
protocol: RC5
address: 00 00 00 00
command: 10 00 00 00
# 
name: VOL-
type: parsed
protocol: RC5
address: 00 00 00 00
command: 11 00 00 00
# 
name: Menu
type: parsed
protocol: RC5
address: 00 00 00 00
command: 2E 00 00 00
# 
name: F1
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 1E 00 00 00
# 
name: F2
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 1F 00 00 00
# 
name: F3
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 20 00 00 00
# 
name: F4
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 21 00 00 00
# 
name: F5
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 22 00 00 00
# 
name: F6
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 23 00 00 00
# 
name: F7
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 24 00 00 00
# 
name: F8
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 25 00 00 00
# 
name: F9
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 26 00 00 00
# 
name: F10
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 27 00 00 00
# 
name: F11
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 28 00 00 00
# 
name: F12
type: parsed
protocol: RC5X
address: 00 00 00 00
command: 29 00 00 00
