Filetype: IR signals file
Version: 1
#
name: LD
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 3F 00 00 00
#
name: LASER_DISC
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 3F 00 00 00
#
name: INPUT:_LD
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 3F 00 00 00
#
name: LD_DISC_B/-
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 72 00 00 00
#
name: LD_DISC_+/A
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 73 00 00 00
