Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 09 00 00 00
#
name: BACKSPACE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0A 00 00 00
#
name: KPENTER
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0C 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0D 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0E 00 00 00
#
name: COMPOSE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 11 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 12 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 13 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 14 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 15 00 00 00
#
name: PLAYCD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 16 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 17 00 00 00
#
name: PAUSECD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 18 00 00 00
#
name: STOPCD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 19 00 00 00
#
name: NEXTSONG
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1A 00 00 00
#
name: PREVIOUSSONG
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1B 00 00 00
#
name: KPSLASH
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1C 00 00 00
#
name: KPASTERISK
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1D 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1E 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1F 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 20 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 21 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 22 00 00 00
#
name: ESC
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 23 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 24 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 25 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 26 00 00 00
#
name: TV2
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 48 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 5A 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 5B 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 5C 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 5D 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 5E 00 00 00
