Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 01 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 01 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 01 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 01 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 01 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 01 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 01 00 00 00
command: 09 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0A 00 00 00
#
name: Jump
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0C 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0F 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 10 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 12 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 14 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 16 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 18 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1A 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1B 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1C 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1D 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1E 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 01 00 00 00
command: 20 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 21 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 01 00 00 00
command: 22 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 01 00 00 00
command: 23 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 24 00 00 00
#
name: ReturnToLive
type: parsed
protocol: NECext
address: 01 00 00 00
command: 25 00 00 00
#
name: SkipAhead
type: parsed
protocol: NECext
address: 01 00 00 00
command: 26 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 01 00 00 00
command: 27 00 00 00
#
name: ReplayGuide
type: parsed
protocol: NECext
address: 01 00 00 00
command: 28 00 00 00
#
name: Zones
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2A 00 00 00
#
name: Input
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2B 00 00 00
