Filetype: IR signals file
Version: 1
#
name: SETUP
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 01 00 00 00
#
name: PLII_NEO6
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 02 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 03 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 04 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 06 00 00 00
#
name: TEST_TONE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 07 00 00 00
#
name: DSP_MODE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 09 00 00 00
#
name: BASS_TREBLE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 0A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 0C 00 00 00
#
name: CH_SELECT
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 0D 00 00 00
#
name: STEREO_MONO
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 0E 00 00 00
#
name: X_1_DIRECT
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 0F 00 00 00
#
name: I-O
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 11 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 12 00 00 00
#
name: DYNAMIC
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 13 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 14 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 15 00 00 00
#
name: PTY
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 16 00 00 00
#
name: DDEX_DTSES
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 17 00 00 00
#
name: STEREO
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1A 00 00 00
#
name: APS
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1B 00 00 00
#
name: TUNER_AM_FM
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1C 00 00 00
#
name: STORE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1D 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 1F 00 00 00
#
name: LFE_TRIM
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 20 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 21 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 22 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 23 00 00 00
#
name: X_VIDEO2
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 24 00 00 00
#
name: X_VIDEO3
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 25 00 00 00
#
name: TAPE_MD_CDR
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 26 00 00 00
#
name: CD_AUX
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 27 00 00 00
#
name: INPUT_MODE
type: parsed
protocol: NECext
address: C0 C0 00 00
command: 60 00 00 00
#
name: DELAY
type: parsed
protocol: NECext
address: C0 C0 00 00
command: A0 00 00 00
