Filetype: IR signals file
Version: 1
#
name: [2]_CHANNEL_^
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 00 00 00 00
#
name: [2]_CHANNEL_V
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 01 00 00 00
#
name: [2]_SLOW_+
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 02 00 00 00
#
name: [2]_SLOW_-
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 03 00 00 00
#
name: [2]_CANCEL/STOP_[]
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 04 00 00 00
#
name: [2]_ENTER/PLAY_>
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 05 00 00 00
#
name: [2]_REC
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 06 00 00 00
#
name: [2]_POWER
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 08 00 00 00
#
name: [2]_RESET
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 09 00 00 00
#
name: [2]_VCR/TV
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 0A 00 00 00
#
name: [2]_FF/SRCH_>>
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 0C 00 00 00
#
name: [2]_REW/SRCH_<<
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 0D 00 00 00
#
name: [2]_PAUSE/STILL_
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 0E 00 00 00
#
name: [2]_1
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 10 00 00 00
#
name: [2]_2
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 11 00 00 00
#
name: [2]_3
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 12 00 00 00
#
name: [2]_4
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 13 00 00 00
#
name: [2]_5
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 14 00 00 00
#
name: [2]_6
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 15 00 00 00
#
name: [2]_7
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 16 00 00 00
#
name: [2]_8
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 17 00 00 00
#
name: [2]_9
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 18 00 00 00
#
name: [2]_0
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 1A 00 00 00
#
name: [2]_SP/EP
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 1B 00 00 00
#
name: [2]_SEARCH_INDEX
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 62 00 00 00
#
name: [2]_TAPE_RETURN
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 72 00 00 00
#
name: [2]_INDEX_WRITE
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 75 00 00 00
#
name: [2]_INDEX_ERASE
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 76 00 00 00
#
name: [2]_ADDRESS
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 84 00 00 00
#
name: [2]_TAPE_REMAIN
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 85 00 00 00
#
name: [2]_SEARCH_TIME
type: parsed
protocol: NECext
address: 19 E7 00 00
command: 9D 00 00 00
#
name: [2]_CVC
type: parsed
protocol: NECext
address: 19 E7 00 00
command: EF 00 00 00
