Filetype: IR signals file
Version: 1
#
name: CH0
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 00 00 00 00
#
name: CH1
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 01 00 00 00
#
name: CH2
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 02 00 00 00
#
name: CH3
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 03 00 00 00
#
name: CH4
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 04 00 00 00
#
name: CH5
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 05 00 00 00
#
name: CH6
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 06 00 00 00
#
name: CH7
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 07 00 00 00
#
name: CH8
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 08 00 00 00
#
name: CH9
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 09 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 0A 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 0B 00 00 00
#
name: TIMER_REC
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 0D 00 00 00
#
name: AUDIOSELECT
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 0E 00 00 00
#
name: CH10+
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 0F 00 00 00
#
name: TVVCR
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 12 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 13 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 14 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 15 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 16 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 17 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 18 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 19 00 00 00
#
name: PAUSESTILL
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 1A 00 00 00
#
name: SHOWVIEW
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 1D 00 00 00
#
name: SPEEDSPLP
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 1E 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 45 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 4A 00 00 00
#
name: COUNTERMEMORY
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 4B 00 00 00
#
name: COUNTERRESET
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 4C 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 4E 00 00 00
#
name: AUDIODUBBING
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 4F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 50 00 00 00
#
name: CLOCKCOUNTER
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 51 00 00 00
#
name: ATR
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 52 00 00 00
#
name: CALL
type: parsed
protocol: NECext
address: 80 7B 00 00
command: 5F 00 00 00
