Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: F11
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: t-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: pp
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: p-p
type: parsed
protocol: NECext
address: 00 00 00 00
command: 22 00 00 00
#
name: iii
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: M
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: f+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: f-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3B 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
