Filetype: IR signals file
Version: 1
#
name: PAGEUP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: PAGEDOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 06 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 07 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 08 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 09 00 00 00
#
name: SWITCHVIDEOMODE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 04 00 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 00 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 00 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 00 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 00 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 00 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 00 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 00 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 00 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 00 00 00
command: 19 00 00 00
#
name: CHANNEL
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1A 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1E 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 20 00 00 00
#
name: CONFIG
type: parsed
protocol: NECext
address: 04 00 00 00
command: 21 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 04 00 00 00
command: 28 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 40 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 41 00 00 00
#
name: MYAPPS
type: parsed
protocol: NECext
address: 04 00 00 00
command: 42 00 00 00
#
name: OPTION
type: parsed
protocol: NECext
address: 04 00 00 00
command: 43 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 04 00 00 00
command: 44 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 00 00 00
command: 45 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 04 00 00 00
command: 53 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5B 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 61 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 04 00 00 00
command: 63 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 71 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 04 00 00 00
command: 72 00 00 00
#
name: PROPS
type: parsed
protocol: NECext
address: 04 00 00 00
command: 79 00 00 00
#
name: HOME
type: parsed
protocol: NECext
address: 04 00 00 00
command: 7C 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 8E 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 04 00 00 00
command: 8F 00 00 00
#
name: APP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 9F 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 04 00 00 00
command: AA 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 04 00 00 00
command: AB 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 04 00 00 00
command: B0 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 04 00 00 00
command: B1 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 04 00 00 00
command: BA 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 04 00 00 00
command: BD 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 04 00 00 00
command: F0 00 00 00
