Filetype: IR signals file
Version: 1
# 
# Edifier R2000DB Audio Receiver
#
name: Power
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 00 FF 00 00
#
name: CLASSIC
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 0E F1 00 00
# 
name: DYNAMIC
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 14 EB 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 0C F3 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 09 F6 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 01 FE 00 00
# 
name: LINE1
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 0D F2 00 00
# 
name: LINE2
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 16 E9 00 00
# 
name: BT
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 15 EA 00 00
# 
name: OPTIC
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 0A F5 00 00
