Filetype: IR signals file
Version: 1
#
name: TV_INPUT
type: parsed
protocol: NECext
address: 50 00 00 00
command: 09 00 00 00
#
name: TV_MUTE
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0B 00 00 00
#
name: TV_VOL_+
type: parsed
protocol: NECext
address: 50 00 00 00
command: 12 00 00 00
#
name: TV_VOL_-
type: parsed
protocol: NECext
address: 50 00 00 00
command: 15 00 00 00
