Filetype: IR signals file
Version: 1
#
name: PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 00 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 01 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 02 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 03 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 04 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 05 00 00 00
#
name: DECK_A/B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 06 00 00 00
#
name: DIR_A
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 07 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 08 00 00 00
#
name: PAUSE_STOP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 09 00 00 00
#
name: SKIP-FFWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0A 00 00 00
#
name: SKIP-REWIND
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0B 00 00 00
#
name: SEARCH_FFWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0C 00 00 00
#
name: SEARCH_REWIND
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0D 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1F 00 00 00
#
name: DIR_B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 40 00 00 00
#
name: DISC-SCAN
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 4F 00 00 00
