Filetype: IR signals file
Version: 1
# 
# Sennheiser Ambeo Soundbar
#
name: Power
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0B 00 00 00
# 
name: Vol_up
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0D 00 00 00
# 
name: Vol_dn
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0E 00 00 00
# 
name: Source_up
type: parsed
protocol: RC5
address: 13 00 00 00
command: 11 00 00 00
# 
name: Source_down
type: parsed
protocol: RC5
address: 13 00 00 00
command: 12 00 00 00
# 
name: Night
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 20 00 00 00
# 
name: Mute
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0C 00 00 00
# 
name: Neutral
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 1F 00 00 00
# 
name: News
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 1D 00 00 00
# 
name: Movie
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 1B 00 00 00
# 
name: Music
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 1C 00 00 00
# 
name: Sport
type: parsed
protocol: RC5X
address: 13 00 00 00
command: 1E 00 00 00
# 
name: Ambeo
type: parsed
protocol: RC5
address: 13 00 00 00
command: 14 00 00 00
# 
name: Record
type: parsed
protocol: RC5
address: 13 00 00 00
command: 35 00 00 00
