Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 00 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: B0 00 00 00
command: 01 00 00 00
#
name: SEARCH_BACK
type: parsed
protocol: NECext
address: B0 00 00 00
command: 04 00 00 00
#
name: SEARCH_FORWARD
type: parsed
protocol: NECext
address: B0 00 00 00
command: 05 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 06 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 0A 00 00 00
#
name: DISC_1
type: parsed
protocol: NECext
address: B0 00 00 00
command: 10 00 00 00
#
name: DISC_2
type: parsed
protocol: NECext
address: B0 00 00 00
command: 11 00 00 00
#
name: DISC_3
type: parsed
protocol: NECext
address: B0 00 00 00
command: 12 00 00 00
#
name: DISC_4
type: parsed
protocol: NECext
address: B0 00 00 00
command: 13 00 00 00
#
name: DISC_5
type: parsed
protocol: NECext
address: B0 00 00 00
command: 14 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: B0 00 00 00
command: 15 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: B0 00 00 00
command: 16 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: B0 00 00 00
command: 17 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: B0 00 00 00
command: 18 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: B0 00 00 00
command: 19 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: B0 00 00 00
command: 33 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B0 00 00 00
command: 3D 00 00 00
#
name: POSITION_MEMORY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 46 00 00 00
#
name: A-B_REPEAT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 48 00 00 00
#
name: SKIP_BACK
type: parsed
protocol: NECext
address: B0 00 00 00
command: 49 00 00 00
#
name: SKIP_FORWARD
type: parsed
protocol: NECext
address: B0 00 00 00
command: 4A 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: B0 00 00 00
command: 4D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: B0 00 00 00
command: 80 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: B0 00 00 00
command: 81 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: B0 00 00 00
command: 82 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: B0 00 00 00
command: 83 00 00 00
#
name: ARROW_UP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 85 00 00 00
#
name: ARROW_DOWN
type: parsed
protocol: NECext
address: B0 00 00 00
command: 86 00 00 00
#
name: ARROW_LEFT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 87 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 88 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 88 00 00 00
#
name: X_0+
type: parsed
protocol: NECext
address: B0 00 00 00
command: 89 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8A 00 00 00
#
name: QUICK_REPLAY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8B 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8C 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 90 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 91 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 92 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 94 00 00 00
#
name: TOP_MENU
type: parsed
protocol: NECext
address: B0 00 00 00
command: 9B 00 00 00
#
name: A_SRD
type: parsed
protocol: NECext
address: B0 00 00 00
command: 9E 00 00 00
#
name: FL_SELECT
type: parsed
protocol: NECext
address: B0 00 00 00
command: B6 00 00 00
#
name: DISC
type: parsed
protocol: NECext
address: B0 00 00 00
command: B7 00 00 00
#
name: SEQUENTIAL
type: parsed
protocol: NECext
address: B0 00 00 00
command: BF 00 00 00
#
name: CINEMA
type: parsed
protocol: NECext
address: B0 00 00 00
command: C0 00 00 00
#
name: BASS
type: parsed
protocol: NECext
address: B0 00 00 00
command: D4 00 00 00
#
name: D_ENH
type: parsed
protocol: NECext
address: B0 00 00 00
command: D5 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: B0 00 00 00
command: EB 00 00 00
