Filetype: IR signals file
Version: 1
#
# UPSTAR TV1
# Autogenerated from ircodes/UPSTAR/TV1.xml
#
name: POWER
type: parsed
protocol: NECext
address: 7C 80 00 00
command: AF 50 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 0F F0 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 7C 80 00 00
command: F5 0A 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 2F D0 00 00
#
name: INPUT TV
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 6D 92 00 00
#
name: INPUT USB
type: parsed
protocol: NECext
address: 7C 80 00 00
command: ED 12 00 00
#
name: 1
type: parsed
protocol: NECext
address: 7C 80 00 00
command: B7 48 00 00
#
name: 2
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 1F E0 00 00
#
name: 3
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 37 C8 00 00
#
name: 4
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 97 68 00 00
#
name: 5
type: parsed
protocol: NECext
address: 7C 80 00 00
command: BF 40 00 00
#
name: 6
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 17 E8 00 00
#
name: 7
type: parsed
protocol: NECext
address: 7C 80 00 00
command: A7 58 00 00
#
name: 8
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 3F C0 00 00
#
name: 9
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 27 D8 00 00
#
name: ADD/DEL
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 8D 72 00 00
#
name: 0
type: parsed
protocol: NECext
address: 7C 80 00 00
command: F7 08 00 00
#
name: CC
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 8F 70 00 00
#
name: FAV+
type: parsed
protocol: NECext
address: 7C 80 00 00
command: CD 32 00 00
#
name: FAV
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 0D F2 00 00
#
name: FAV-
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 4D B2 00 00
#
name: FORMATS
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 55 AA 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 45 BA 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 7C 80 00 00
command: D5 2A 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 35 CA 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 87 78 00 00
#
name: UP
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 85 7A 00 00
#
name: CH+
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 07 F8 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 25 DA 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 7C 80 00 00
command: A5 5A 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 7C 80 00 00
command: E5 1A 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 05 FA 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 95 6A 00 00
#
name: CH-
type: parsed
protocol: NECext
address: 7C 80 00 00
command: C5 3A 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 15 EA 00 00
#
name: MTS/SAP
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 9F 60 00 00
#
name: LAST CH
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 75 8A 00 00
#
name: PICTURE
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 2D D2 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 7C 80 00 00
command: 65 9A 00 00
#
name: SOUND
type: parsed
protocol: NECext
address: 7C 80 00 00
command: AD 52 00 00
