Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0A 00 00 00
#
name: TV/TXT
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0B 00 00 00
#
name: TV/AV
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0C 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0D 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0F 00 00 00
#
name: PICTURE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 10 00 00 00
#
name: info+
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 11 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 11 00 00 00
#
name: EXP.
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 13 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 14 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 15 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 16 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 17 00 00 00
#
name: NORM
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 18 00 00 00
#
name: HOLD
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 18 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 19 00 00 00
#
name: MIX
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1A 00 00 00
#
name: REV
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1B 00 00 00
#
name: R
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1C 00 00 00
#
name: G
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1D 00 00 00
#
name: Y
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1E 00 00 00
#
name: C
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1F 00 00 00
