Filetype: IR signals file
Version: 1
# 
# RCA TV RT2471-AC 
#
name: Power
type: parsed
protocol: NEC
address: A0 00 00 00
command: 5F 00 00 00
# 
name: Input
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1A 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: A0 00 00 00
command: 13 00 00 00
# 
name: Info
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1B 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: A0 00 00 00
command: 10 00 00 00
# 
name: Ok
type: parsed
protocol: NEC
address: A0 00 00 00
command: 55 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: A0 00 00 00
command: 59 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: A0 00 00 00
command: 51 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: A0 00 00 00
command: 56 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: A0 00 00 00
command: 14 00 00 00
# 
name: Next
type: parsed
protocol: NEC
address: A0 00 00 00
command: 49 00 00 00
# 
name: Prev
type: parsed
protocol: NEC
address: A0 00 00 00
command: 4A 00 00 00
# 
name: Fast_fo
type: parsed
protocol: NEC
address: A0 00 00 00
command: 08 00 00 00
# 
name: Fast_ba
type: parsed
protocol: NEC
address: A0 00 00 00
command: 09 00 00 00
# 
name: Play_pa
type: parsed
protocol: NEC
address: A0 00 00 00
command: 4D 00 00 00
# 
name: Pause
type: parsed
protocol: NEC
address: A0 00 00 00
command: 4D 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: A0 00 00 00
command: 4D 00 00 00
# 
name: Stop
type: parsed
protocol: NEC
address: A0 00 00 00
command: 0D 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1C 00 00 00
# 
name: Mode
type: parsed
protocol: NEC
address: A0 00 00 00
command: 5A 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: A0 00 00 00
command: 40 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: A0 00 00 00
command: 5D 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: A0 00 00 00
command: 03 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1F 00 00 00
