Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: 03 00 00 00
command: 00 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 03 00 00 00
command: 04 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 03 00 00 00
command: 05 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 03 00 00 00
command: 0B 00 00 00
#
name: AV_STATUS
type: parsed
protocol: NECext
address: 03 00 00 00
command: 0D 00 00 00
#
name: CC
type: parsed
protocol: NECext
address: 03 00 00 00
command: 0E 00 00 00
#
name: TV/VIDEO
type: parsed
protocol: NECext
address: 03 00 00 00
command: 13 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 03 00 00 00
command: 17 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 03 00 00 00
command: 18 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 03 00 00 00
command: 19 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 03 00 00 00
command: 1C 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 03 00 00 00
command: 1E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 03 00 00 00
command: 1F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 03 00 00 00
command: 20 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 03 00 00 00
command: 21 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 03 00 00 00
command: 22 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 03 00 00 00
command: 23 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 03 00 00 00
command: 24 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 03 00 00 00
command: 25 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 03 00 00 00
command: 26 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 03 00 00 00
command: 27 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 03 00 00 00
command: 28 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 03 00 00 00
command: 29 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 03 00 00 00
command: 3C 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: 03 00 00 00
command: 5A 00 00 00
#
name: ARROW_LEFT
type: parsed
protocol: NECext
address: 03 00 00 00
command: 5B 00 00 00
#
name: X_0+
type: parsed
protocol: NECext
address: 03 00 00 00
command: 77 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 03 00 00 00
command: 7A 00 00 00
#
name: ARROW_DOWN
type: parsed
protocol: NECext
address: 03 00 00 00
command: 7B 00 00 00
#
name: ARROW_UP
type: parsed
protocol: NECext
address: 03 00 00 00
command: 7C 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 03 00 00 00
command: 89 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 03 00 00 00
command: B2 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 03 00 00 00
command: D6 00 00 00
#
name: C1/C2
type: parsed
protocol: NECext
address: 03 00 00 00
command: DA 00 00 00
