Filetype: IR signals file
Version: 1
# 
# Manta TV 2
#
name: Power
type: parsed
protocol: NEC
address: A0 00 00 00
command: 5F 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: A0 00 00 00
command: 40 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: A0 00 00 00
command: 5D 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: A0 00 00 00
command: 03 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1F 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1C 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1A 00 00 00
# 
name: Ok
type: parsed
protocol: NEC
address: A0 00 00 00
command: 55 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: A0 00 00 00
command: 59 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: A0 00 00 00
command: 51 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: A0 00 00 00
command: 56 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: A0 00 00 00
command: 14 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: A0 00 00 00
command: 13 00 00 00
# 
name: Exit
type: parsed
protocol: NEC
address: A0 00 00 00
command: 10 00 00 00
