Filetype: IR signals file
Version: 1
# 
# Gigabyte AORUS TV Monitor
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1A 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 33 00 00 00
