Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 06 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 06 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 06 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 06 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 06 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 06 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 06 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 06 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 06 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 06 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 06 00 00 00
command: 15 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 06 00 00 00
command: 18 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 06 00 00 00
command: 19 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 06 00 00 00
command: 1A 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 06 00 00 00
command: 1E 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 06 00 00 00
command: 1F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 06 00 00 00
command: 2B 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 06 00 00 00
command: 2C 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 06 00 00 00
command: 34 00 00 00
#
name: ChnDn
type: parsed
protocol: NECext
address: 06 00 00 00
command: 35 00 00 00
#
name: Ent
type: parsed
protocol: NECext
address: 06 00 00 00
command: 39 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 06 00 00 00
command: 3F 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 06 00 00 00
command: 64 00 00 00
#
name: AB
type: parsed
protocol: NECext
address: 06 00 00 00
command: 70 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 06 00 00 00
command: 7F 00 00 00
