Filetype: IR signals file
Version: 1
#
name: PauseStep
type: parsed
protocol: NECext
address: 45 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 45 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 45 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 45 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 45 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 45 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 45 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 45 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 45 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 45 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 45 00 00 00
command: 0A 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 45 00 00 00
command: 0D 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 45 00 00 00
command: 12 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 45 00 00 00
command: 13 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 45 00 00 00
command: 14 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 45 00 00 00
command: 15 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 45 00 00 00
command: 16 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 45 00 00 00
command: 19 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 45 00 00 00
command: 20 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 45 00 00 00
command: 21 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 45 00 00 00
command: 22 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 45 00 00 00
command: 23 00 00 00
#
name: SkipForward
type: parsed
protocol: NECext
address: 45 00 00 00
command: 24 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 45 00 00 00
command: 25 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 45 00 00 00
command: 26 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 45 00 00 00
command: 27 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 45 00 00 00
command: 28 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 45 00 00 00
command: 29 00 00 00
#
name: Memory
type: parsed
protocol: NECext
address: 45 00 00 00
command: 2A 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 45 00 00 00
command: 2B 00 00 00
#
name: RepeatA-B
type: parsed
protocol: NECext
address: 45 00 00 00
command: 2C 00 00 00
#
name: Random
type: parsed
protocol: NECext
address: 45 00 00 00
command: 2E 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 45 00 00 00
command: 40 00 00 00
#
name: FlDim
type: parsed
protocol: NECext
address: 45 00 00 00
command: 41 00 00 00
#
name: EAM
type: parsed
protocol: NECext
address: 45 00 00 00
command: 43 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 45 00 00 00
command: 4D 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 45 00 00 00
command: 51 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 45 00 00 00
command: 80 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 45 00 00 00
command: 81 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 45 00 00 00
command: 84 00 00 00
#
name: FlSelect
type: parsed
protocol: NECext
address: 45 00 00 00
command: D7 00 00 00
#
name: TopMenu
type: parsed
protocol: NECext
address: 45 00 00 00
command: DE 00 00 00
#
name: EPM
type: parsed
protocol: NECext
address: 45 00 00 00
command: EE 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 45 00 00 00
command: EF 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 45 00 00 00
command: F5 00 00 00
