Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: PICTURE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: I
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 18 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 22 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: AD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 24 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 25 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 27 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 28 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: CHAPTER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: PIP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2F 00 00 00
#
name: ZOOMOUT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 30 00 00 00
#
name: ZOOMIN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 31 00 00 00
#
name: CAPTURE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: WWW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 33 00 00 00
#
name: EMAIL
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: PHONE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
