Filetype: IR signals file
Version: 1
#
name: EJECTCD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 00 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 01 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 02 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 03 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 04 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 05 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 06 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 07 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 08 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 09 00 00 00
#
name: p/still
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0B 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0C 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0D 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0E 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 16 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 18 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 19 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1C 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1D 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1E 00 00 00
#
name: clear/reset
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1F 00 00 00
#
name: timer-prog
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 3A 00 00 00
#
name: viss
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 41 00 00 00
#
name: trk-
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 44 00 00 00
#
name: trk+
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 45 00 00 00
#
name: clock/count
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 4C 00 00 00
#
name: tv/av
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 56 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 58 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 59 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 5C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 5D 00 00 00
#
name: auto
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 5F 00 00 00
#
name: qview
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 77 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 7D 00 00 00
#
name: system
type: parsed
protocol: NECext
address: 6E 00 00 00
command: DC 00 00 00
