Filetype: IR signals file
Version: 1
#
name: ANTENNA
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 05 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 06 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 08 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 08 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0C 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0C 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 12 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1A 00 00 00
#
name: PIP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1B 00 00 00
#
name: PIP_AUDIO_MONITOR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1B 00 00 00
#
name: ID
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1E 00 00 00
#
name: PREVIOUS_CHANNEL
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: PREV_CH
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 31 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 31 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 32 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 32 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 35 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 35 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 36 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 36 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 37 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 37 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 38 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 38 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 39 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 39 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3A 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3A 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3A 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3B 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3B 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3C 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: CS
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 53 00 00 00
#
name: SKIP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 53 00 00 00
#
name: MOVE_LEFT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 56 00 00 00
#
name: MOVE_RIGHT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 57 00 00 00
#
name: MOVE_DOWN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 58 00 00 00
#
name: MOVE_UP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 59 00 00 00
#
name: SURROUND
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 5A 00 00 00
#
name: MENU_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 64 00 00 00
#
name: MENU_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 65 00 00 00
#
name: CINEMA
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 90 00 00 00
#
name: SPLIT_SCREEN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 91 00 00 00
#
name: SPLIT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 91 00 00 00
#
name: POP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 92 00 00 00
#
name: FETCH
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 93 00 00 00
#
name: INPUT_SOURCE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: A3 00 00 00
#
name: INPUT_SOURCE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: A3 00 00 00
#
name: SWAP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: C3 00 00 00
#
name: SWAP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: C3 00 00 00
#
name: SCAN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: C4 00 00 00
#
name: SIZE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: C5 00 00 00
#
name: CH_CTRL
type: parsed
protocol: NECext
address: 0F 00 00 00
command: E5 00 00 00
