Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0C 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0F 00 00 00
#
name: S/REWIND
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0F 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 28 00 00 00
#
name: S/AV
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 28 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2F 00 00 00
#
name: S/PLAY
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2F 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 46 00 00 00
#
name: S/MUTE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 46 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 4F 00 00 00
#
name: S/FORWARD
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 4F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 50 00 00 00
#
name: S/P+
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 50 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 51 00 00 00
#
name: S/P-
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 51 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 52 00 00 00
#
name: S/STOP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 52 00 00 00
#
name: 2-
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 53 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 55 00 00 00
#
name: S/VOL-
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 55 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 56 00 00 00
#
name: S/VOL+
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 56 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 57 00 00 00
#
name: S/OK
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 57 00 00 00
#
name: 1-/--
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 61 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6A 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6A 00 00 00
#
name: S/MENU
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6A 00 00 00
#
name: S/PAUSE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6A 00 00 00
#
name: F1
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6B 00 00 00
#
name: S/F1
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6B 00 00 00
#
name: F2
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6C 00 00 00
#
name: S/F2
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6C 00 00 00
#
name: F3
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6D 00 00 00
#
name: S/F3
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6D 00 00 00
#
name: F4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6E 00 00 00
#
name: S/F4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6E 00 00 00
#
name: TVf4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6F 00 00 00
