Filetype: IR signals file
Version: 1
# 
# LG SPECIAL HOTEL TV REMOTE
#
# by JEREMYNO
#
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: Ok
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
# 
name: Exit
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5B 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 04 00 00 00
command: 11 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 04 00 00 00
command: 14 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 04 00 00 00
command: 15 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 04 00 00 00
command: 17 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 04 00 00 00
command: 18 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 04 00 00 00
command: 19 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 04 00 00 00
command: 10 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 04 00 00 00
command: 28 00 00 00
# 
name: Txt
type: parsed
protocol: NEC
address: 04 00 00 00
command: 20 00 00 00
# 
name: Red
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Yelow
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: Green
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Blue
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: 04 00 00 00
command: 00 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: 04 00 00 00
command: 01 00 00 00
# 
name: I
type: parsed
protocol: NEC
address: 04 00 00 00
command: AA 00 00 00
# 
name: Tv
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 174 119830 169
# 
name: Av
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
# 
name: Dtt
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 174 39827 177 19824 178 19823 168 19830 172 39829 175
