Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 00 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 01 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 02 00 00 00
#
name: activebass
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 04 00 00 00
#
name: band
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 0B 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 0D 00 00 00
#
name: fmstereo
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 1F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 21 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 22 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 23 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 24 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 25 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 26 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 27 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 28 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 29 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 2A 00 00 00
#
name: X_0+
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 2E 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 32 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 3D 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 3E 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 42 00 00 00
#
name: counterreset
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 57 00 00 00
#
name: deckab
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 58 00 00 00
#
name: revmode
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 5F 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 70 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 71 00 00 00
#
name: program
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 74 00 00 00
#
name: random
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 77 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 78 00 00 00
#
name: allcdeject
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 7B 00 00 00
#
name: continue
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 7D 00 00 00
#
name: sound
type: parsed
protocol: NECext
address: 9F 00 00 00
command: 8F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F1 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F2 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F3 00 00 00
#
name: ejectcd1
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F4 00 00 00
#
name: ejectcd2
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F5 00 00 00
#
name: ejectcd3
type: parsed
protocol: NECext
address: 9F 00 00 00
command: F6 00 00 00
