Filetype: IR signals file
Version: 1
# 
name: Power
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0F F0 00 00
# 
name: Input
type: parsed
protocol: NECext
address: 86 05 00 00
command: 1D E2 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0C F3 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0D F2 00 00
# 
name: Ch_next
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0A F5 00 00
# 
name: Ch_prev
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0B F4 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0E F1 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 86 05 00 00
command: 14 EB 00 00
# 
name: Exit
type: parsed
protocol: NECext
address: 86 05 00 00
command: 1B E4 00 00
# 
name: Info
type: parsed
protocol: NECext
address: 86 05 00 00
command: 17 E8 00 00
# 
name: Guide
type: parsed
protocol: NECext
address: 86 05 00 00
command: 45 BA 00 00
# 
name: Enter
type: parsed
protocol: NECext
address: 86 05 00 00
command: 18 E7 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 86 05 00 00
command: 42 BD 00 00
# 
name: Dn
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 8990 3428 197 822 619 543 590 1670 596 1663 592 545 588 550 593 544 589 549 594 1665 590 1668 587 550 593 1666 589 548 595 543 590 548 595 542 591 547 596 1663 592 1666 589 548 595 542 591 547 596 541 592 1668 587 549 594 544 589 548 595 1665 590 1668 587 1671 595 1665 590 547 596 1663 592 42384 8983 2211 621
# 
name: Left
type: parsed
protocol: NECext
address: 86 05 00 00
command: 16 E9 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 86 05 00 00
command: 15 EA 00 00
# 
name: Favorite
type: parsed
protocol: NECext
address: 86 05 00 00
command: 4B B4 00 00
# 
name: Video
type: parsed
protocol: NECext
address: 86 05 00 00
command: 4C B3 00 00
# 
name: Hdmi
type: parsed
protocol: NECext
address: 86 05 00 00
command: 50 AF 00 00
# 
name: Tv
type: parsed
protocol: NECext
address: 86 05 00 00
command: 4F B0 00 00
# 
name: Comp
type: parsed
protocol: NECext
address: 86 05 00 00
command: 4D B2 00 00
# 
name: Mts_sap
type: parsed
protocol: NECext
address: 86 05 00 00
command: 11 EE 00 00
# 
name: Vga
type: parsed
protocol: NECext
address: 86 05 00 00
command: 4E B1 00 00
# 
name: Zoom
type: parsed
protocol: NECext
address: 86 05 00 00
command: 44 BB 00 00
# 
name: Sleep
type: parsed
protocol: NECext
address: 86 05 00 00
command: 13 EC 00 00
# 
name: Ch_list
type: parsed
protocol: NECext
address: 86 05 00 00
command: 86 79 00 00
# 
name: Picture
type: parsed
protocol: NECext
address: 86 05 00 00
command: 49 B6 00 00
# 
name: Audio
type: parsed
protocol: NECext
address: 86 05 00 00
command: 48 B7 00 00
# 
name: Ccd
type: parsed
protocol: NECext
address: 86 05 00 00
command: 1C E3 00 00
# 
name: 1
type: parsed
protocol: NECext
address: 86 05 00 00
command: 00 FF 00 00
# 
name: 2
type: parsed
protocol: NECext
address: 86 05 00 00
command: 01 FE 00 00
# 
name: 3
type: parsed
protocol: NECext
address: 86 05 00 00
command: 02 FD 00 00
# 
name: 4
type: parsed
protocol: NECext
address: 86 05 00 00
command: 03 FC 00 00
# 
name: 5
type: parsed
protocol: NECext
address: 86 05 00 00
command: 01 FE 00 00
# 
name: 6
type: parsed
protocol: NECext
address: 86 05 00 00
command: 05 FA 00 00
# 
name: 7
type: parsed
protocol: NECext
address: 86 05 00 00
command: 06 F9 00 00
# 
name: 8
type: parsed
protocol: NECext
address: 86 05 00 00
command: 07 F8 00 00
# 
name: 9
type: parsed
protocol: NECext
address: 86 05 00 00
command: 08 F7 00 00
# 
name: 0
type: parsed
protocol: NECext
address: 86 05 00 00
command: 09 F6 00 00
# 
name: Dot
type: parsed
protocol: NECext
address: 86 05 00 00
command: 41 BE 00 00
# 
name: Recall
type: parsed
protocol: NECext
address: 86 05 00 00
command: 10 EF 00 00
