Filetype: IR signals file
Version: 1
#
name: RADIO
type: parsed
protocol: NECext
address: 48 00 00 00
command: 00 00 00 00
#
name: am
type: parsed
protocol: NECext
address: 48 00 00 00
command: 01 00 00 00
#
name: t_up
type: parsed
protocol: NECext
address: 48 00 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 48 00 00 00
command: 04 00 00 00
#
name: t_down
type: parsed
protocol: NECext
address: 48 00 00 00
command: 05 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 48 00 00 00
command: 07 00 00 00
#
name: v_down
type: parsed
protocol: NECext
address: 48 00 00 00
command: 08 00 00 00
#
name: muting
type: parsed
protocol: NECext
address: 48 00 00 00
command: 09 00 00 00
#
name: cdp_program
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0A 00 00 00
#
name: cdp_play
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0B 00 00 00
#
name: cdp_memory
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0C 00 00 00
#
name: cdp_stop
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0D 00 00 00
#
name: cdp_fskip
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0E 00 00 00
#
name: cdp_bskip
type: parsed
protocol: NECext
address: 48 00 00 00
command: 0F 00 00 00
#
name: phono
type: parsed
protocol: NECext
address: 48 00 00 00
command: 11 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 48 00 00 00
command: 12 00 00 00
