Filetype: IR signals file
Version: 1
# 
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
# 
name: Info
type: parsed
protocol: NEC
address: 04 00 00 00
command: AA 00 00 00
# 
name: Input
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
# 
name: Av_mode
type: parsed
protocol: NEC
address: 04 00 00 00
command: 30 00 00 00
# 
name: Energy
type: parsed
protocol: NEC
address: 04 00 00 00
command: 95 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 04 00 00 00
command: 11 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 04 00 00 00
command: 14 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 04 00 00 00
command: 15 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 04 00 00 00
command: 17 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 04 00 00 00
command: 18 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 04 00 00 00
command: 19 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 04 00 00 00
command: 10 00 00 00
# 
name: _
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4C 00 00 00
# 
name: Flashback
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1A 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: Enter
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: Chann_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 00 00 00 00
# 
name: Chann_down
type: parsed
protocol: NEC
address: 04 00 00 00
command: 01 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 04 00 00 00
command: 43 00 00 00
# 
name: Return
type: parsed
protocol: NEC
address: 04 00 00 00
command: 28 00 00 00
# 
name: Red
type: parsed
protocol: NEC
address: 04 00 00 00
command: 72 00 00 00
# 
name: Green_stop
type: parsed
protocol: NEC
address: 04 00 00 00
command: 71 00 00 00
# 
name: Yell_play
type: parsed
protocol: NEC
address: 04 00 00 00
command: 63 00 00 00
# 
name: Blue_pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: 61 00 00 00
# 
name: Q_menu
type: parsed
protocol: NEC
address: 04 00 00 00
command: 45 00 00 00
# 
name: Reverse
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8F 00 00 00
# 
name: Forward
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8E 00 00 00
# 
name: Simplink
type: parsed
protocol: NEC
address: 04 00 00 00
command: 7E 00 00 00
# 
name: Mark_fav
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1E 00 00 00
