Filetype: IR signals file
Version: 1
# 
# JBL On Stage IIIP Speaker
# 
name: Plus
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 03 FC 00 00
# 
name: Minus
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 01 FE 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 19 E6 00 00
# 
name: Play_pause
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 02 FD 00 00
# 
name: Prev
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 12 ED 00 00
# 
name: Next
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 05 FA 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 1E E1 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 0F F0 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 1A E5 00 00
# 
name: Enter
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 06 F9 00 00
