Filetype: IR signals file
Version: 1
#
name: TAPE_PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 00 00 00 00
#
name: TAPE_REWIND
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 01 00 00 00
#
name: TAPE_FFWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 02 00 00 00
#
name: TAPE_STOP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 03 00 00 00
#
name: TAPE_REC/PAUSE
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 04 00 00 00
#
name: TAPE_REC_MUTE
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 05 00 00 00
#
name: TAPE_DECK_A/B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 06 00 00 00
#
name: TAPE_DIR_A
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 07 00 00 00
#
name: CD_PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 08 00 00 00
#
name: CD_STOP/PAUSE
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 09 00 00 00
#
name: CD_SKIP_FWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0A 00 00 00
#
name: CD_SKIP_REW
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0B 00 00 00
#
name: CD_SEARCH_FWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0C 00 00 00
#
name: CD_SEARCH_REW
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0D 00 00 00
#
name: PHONO_PLAY/CUT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0E 00 00 00
#
name: TUNER_PRESET_+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 10 00 00 00
#
name: TUNER_PRESET_-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 11 00 00 00
#
name: TUNER_A/B/C/D/E
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 12 00 00 00
#
name: PHONO_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 14 00 00 00
#
name: CD_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 15 00 00 00
#
name: TUNER_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 16 00 00 00
#
name: LD_V_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 17 00 00 00
#
name: TAPE_1/DAT_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 18 00 00 00
#
name: VCR_APE_2_SELECT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 19 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1F 00 00 00
#
name: TAPE_DIR_B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 40 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 57 00 00 00
#
name: EQ_ON/FLAT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 5A 00 00 00
#
name: EQ_PRESET_SKIP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 5B 00 00 00
