Filetype: IR signals file
Version: 1
# 
# Hikvision NVR/DVR
#
name: Power
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0C F3 00 00
# 
name: Dev
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1F E0 00 00
# 
name: Rec
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1B E4 00 00
# 
name: Play
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1A E5 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 41 BE 00 00
# 
name: Prev
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1D E2 00 00
# 
name: Info
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 16 E9 00 00
# 
name: VOiP/MON
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 15 EA 00 00
# 
name: UP -Skip
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0D F2 00 00
# 
name: LEFT -REW
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0A F5 00 00
# 
name: RIGHT -FF
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0B F4 00 00
# 
name: DN -PREV
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0E F1 00 00
# 
name: Enter-PP
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 0F F0 00 00
# 
name: PTZ
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1C E3 00 00
# 
name: ESC
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 14 EB 00 00
# 
name: Bk-Pause
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 40 BF 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 42 BD 00 00
# 
name: Plus
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 43 BC 00 00
# 
name: Minus
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 44 BB 00 00
# 
name: Iris +
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 45 BA 00 00
# 
name: Iris -
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 49 B6 00 00
# 
name: Focus +
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 46 B9 00 00
# 
name: Focus -
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 4A B5 00 00
# 
name: Zoom +
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 47 B8 00 00
# 
name: Zoom -
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 4B B4 00 00
# 
name: F1
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 48 B7 00 00
# 
name: F2
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 4C B3 00 00
# 
name: Edit
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 13 EC 00 00
# 
name: A
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 1E E1 00 00
#
name: 0
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 00 FF 00 00
#
name: 1
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 01 FE 00 00
# 
name: 2
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 02 FD 00 00
# 
name: 3
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 03 FC 00 00
# 
name: 4
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 04 FB 00 00
# 
name: 5
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 05 FA 00 00
# 
name: 6
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 06 F9 00 00
# 
name: 7
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 07 F8 00 00
# 
name: 8
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 08 F7 00 00
# 
name: 9
type: parsed
protocol: NECext
address: 01 FF 00 00
command: 09 F6 00 00
