Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 70 00 00 00
command: 00 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 70 00 00 00
command: 0C 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 70 00 00 00
command: 0D 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 70 00 00 00
command: 0E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 70 00 00 00
command: 11 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 70 00 00 00
command: 12 00 00 00
#
name: band
type: parsed
protocol: NECext
address: 70 00 00 00
command: 13 00 00 00
#
name: tape_play
type: parsed
protocol: NECext
address: 70 00 00 00
command: 14 00 00 00
#
name: tape_stop
type: parsed
protocol: NECext
address: 70 00 00 00
command: 15 00 00 00
#
name: tape_next
type: parsed
protocol: NECext
address: 70 00 00 00
command: 16 00 00 00
#
name: tape_prev
type: parsed
protocol: NECext
address: 70 00 00 00
command: 17 00 00 00
#
name: tape_rec
type: parsed
protocol: NECext
address: 70 00 00 00
command: 18 00 00 00
#
name: tape_pause
type: parsed
protocol: NECext
address: 70 00 00 00
command: 19 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 70 00 00 00
command: 1F 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 70 00 00 00
command: 40 00 00 00
#
name: tunermode
type: parsed
protocol: NECext
address: 70 00 00 00
command: 4E 00 00 00
#
name: repet
type: parsed
protocol: NECext
address: 70 00 00 00
command: 51 00 00 00
#
name: memory
type: parsed
protocol: NECext
address: 70 00 00 00
command: 52 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 70 00 00 00
command: 53 00 00 00
#
name: t-standby
type: parsed
protocol: NECext
address: 70 00 00 00
command: 5A 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 70 00 00 00
command: 5D 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 70 00 00 00
command: 80 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 70 00 00 00
command: 91 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 70 00 00 00
command: 92 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 70 00 00 00
command: 93 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 70 00 00 00
command: 94 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 70 00 00 00
command: 95 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 70 00 00 00
command: 96 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 70 00 00 00
command: 97 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 70 00 00 00
command: 98 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 70 00 00 00
command: 99 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 70 00 00 00
command: 9A 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 70 00 00 00
command: 9B 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 70 00 00 00
command: C4 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 70 00 00 00
command: C5 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 70 00 00 00
command: C6 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 70 00 00 00
command: C7 00 00 00
#
name: dimmer
type: parsed
protocol: NECext
address: 70 00 00 00
command: CD 00 00 00
#
name: tray
type: parsed
protocol: NECext
address: 70 00 00 00
command: CF 00 00 00
