Filetype: IR signals file
Version: 1
#
name: MODE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 00 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 00 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 79 00 00 00
command: 00 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 01 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 79 00 00 00
command: 02 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 79 00 00 00
command: 04 00 00 00
#
name: SEARCH_<<
type: parsed
protocol: NECext
address: 79 00 00 00
command: 05 00 00 00
#
name: SEARCH_>>
type: parsed
protocol: NECext
address: 79 00 00 00
command: 06 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 79 00 00 00
command: 07 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 79 00 00 00
command: 08 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 79 00 00 00
command: 0A 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: 79 00 00 00
command: 0B 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 79 00 00 00
command: 0C 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 79 00 00 00
command: 0D 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 79 00 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 79 00 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 79 00 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 79 00 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 79 00 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 79 00 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 79 00 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 79 00 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 79 00 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 79 00 00 00
command: 19 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1A 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1B 00 00 00
#
name: SHUFFLE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1B 00 00 00
#
name: OUTPUT_-
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1C 00 00 00
#
name: OUTPUT_+
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1D 00 00 00
#
name: DIMMER
type: parsed
protocol: NECext
address: 79 00 00 00
command: 1E 00 00 00
#
name: DISC_1
type: parsed
protocol: NECext
address: 79 00 00 00
command: 21 00 00 00
#
name: DISC_2
type: parsed
protocol: NECext
address: 79 00 00 00
command: 22 00 00 00
#
name: DISC_3
type: parsed
protocol: NECext
address: 79 00 00 00
command: 23 00 00 00
#
name: DISC_4
type: parsed
protocol: NECext
address: 79 00 00 00
command: 24 00 00 00
#
name: DISC_5
type: parsed
protocol: NECext
address: 79 00 00 00
command: 25 00 00 00
#
name: DISC_+
type: parsed
protocol: NECext
address: 79 00 00 00
command: 4F 00 00 00
#
name: DISC_-
type: parsed
protocol: NECext
address: 79 00 00 00
command: 50 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 55 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 79 00 00 00
command: 56 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 79 00 00 00
command: 57 00 00 00
#
name: RANDOM_NORMAL
type: parsed
protocol: NECext
address: 79 00 00 00
command: 79 00 00 00
#
name: RANDOM_ON
type: parsed
protocol: NECext
address: 79 00 00 00
command: 7A 00 00 00
#
name: REPEAT_OFF
type: parsed
protocol: NECext
address: 79 00 00 00
command: 7C 00 00 00
#
name: REPEAT_ALL
type: parsed
protocol: NECext
address: 79 00 00 00
command: 7D 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 79 00 00 00
command: 7E 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 79 00 00 00
command: 7F 00 00 00
