Filetype: IR signals file
Version: 1
#
name: VOL+
type: parsed
protocol: NECext
address: 01 F1 00 00
command: 53 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 01 F1 00 00
command: 55 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 01 F1 00 00
command: 59 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 01 F1 00 00
command: 5A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 01 F1 00 00
command: 5D 00 00 00
