Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: A8 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A8 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A8 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A8 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A8 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A8 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A8 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A8 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A8 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A8 00 00 00
command: 09 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: A8 00 00 00
command: 10 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: A8 00 00 00
command: 11 00 00 00
#
name: chp/tm
type: parsed
protocol: NECext
address: A8 00 00 00
command: 13 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: A8 00 00 00
command: 16 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A8 00 00 00
command: 17 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A8 00 00 00
command: 18 00 00 00
#
name: memory
type: parsed
protocol: NECext
address: A8 00 00 00
command: 19 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: A8 00 00 00
command: 19 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1C 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1E 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1F 00 00 00
#
name: display
type: parsed
protocol: NECext
address: A8 00 00 00
command: 43 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: A8 00 00 00
command: 44 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: A8 00 00 00
command: 45 00 00 00
#
name: repeata-b
type: parsed
protocol: NECext
address: A8 00 00 00
command: 48 00 00 00
#
name: pgm
type: parsed
protocol: NECext
address: A8 00 00 00
command: 4C 00 00 00
#
name: step-
type: parsed
protocol: NECext
address: A8 00 00 00
command: 50 00 00 00
#
name: seek+
type: parsed
protocol: NECext
address: A8 00 00 00
command: 52 00 00 00
#
name: seek-
type: parsed
protocol: NECext
address: A8 00 00 00
command: 53 00 00 00
#
name: step+
type: parsed
protocol: NECext
address: A8 00 00 00
command: 54 00 00 00
#
name: multi-speed-
type: parsed
protocol: NECext
address: A8 00 00 00
command: 55 00 00 00
#
name: multi-speed+
type: parsed
protocol: NECext
address: A8 00 00 00
command: 58 00 00 00
#
name: intro
type: parsed
protocol: NECext
address: A8 00 00 00
command: 5A 00 00 00
#
name: random
type: parsed
protocol: NECext
address: A8 00 00 00
command: 5E 00 00 00
