Filetype: IR signals file
Version: 1
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 06 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 07 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 08 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 09 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0A 00 00 00
#
name: tv/video
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0B 00 00 00
#
name: timer
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0E 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 04 00 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 00 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 00 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 00 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 00 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 00 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 00 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 00 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 00 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 00 00 00
command: 19 00 00 00
#
name: flashbk
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1A 00 00 00
#
name: surf
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1E 00 00 00
#
name: cc
type: parsed
protocol: NECext
address: 04 00 00 00
command: 39 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 40 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 41 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 00 00 00
command: 43 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 44 00 00 00
#
name: dash
type: parsed
protocol: NECext
address: 04 00 00 00
command: 4C 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 04 00 00 00
command: 4D 00 00 00
#
name: front
type: parsed
protocol: NECext
address: 04 00 00 00
command: 51 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5B 00 00 00
#
name: pip
type: parsed
protocol: NECext
address: 04 00 00 00
command: 60 00 00 00
#
name: pcin
type: parsed
protocol: NECext
address: 04 00 00 00
command: 61 00 00 00
#
name: swap
type: parsed
protocol: NECext
address: 04 00 00 00
command: 63 00 00 00
#
name: freeze
type: parsed
protocol: NECext
address: 04 00 00 00
command: 65 00 00 00
#
name: pipch+
type: parsed
protocol: NECext
address: 04 00 00 00
command: 71 00 00 00
#
name: pipch-
type: parsed
protocol: NECext
address: 04 00 00 00
command: 72 00 00 00
#
name: ratio
type: parsed
protocol: NECext
address: 04 00 00 00
command: 79 00 00 00
#
name: signal
type: parsed
protocol: NECext
address: 04 00 00 00
command: 96 00 00 00
#
name: comp/dvi
type: parsed
protocol: NECext
address: 04 00 00 00
command: 98 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 04 00 00 00
command: AA 00 00 00
