Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 01 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 02 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 03 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 08 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 09 00 00 00
#
name: A.REPEART
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0A 00 00 00
#
name: STILL/F.ADV
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0B 00 00 00
#
name: TRK+
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 11 00 00 00
#
name: TRK-
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 12 00 00 00
#
name: OPERATE
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 14 00 00 00
#
name: TV/VCR
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 15 00 00 00
#
name: A.TRK
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 17 00 00 00
