Filetype: IR signals file
Version: 1
#
name: PLAY
type: parsed
protocol: NECext
address: 00 99 00 00
command: 00 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 00 99 00 00
command: 01 00 00 00
#
name: Resume
type: parsed
protocol: NECext
address: 00 99 00 00
command: 02 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: 00 99 00 00
command: 04 00 00 00
#
name: TimeSearch
type: parsed
protocol: NECext
address: 00 99 00 00
command: 05 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 99 00 00
command: 06 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 00 99 00 00
command: 07 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 99 00 00
command: 09 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0A 00 00 00
#
name: Digest
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0B 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0C 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0D 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0F 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 99 00 00
command: 11 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 99 00 00
command: 12 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 99 00 00
command: 13 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 99 00 00
command: 14 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 99 00 00
command: 15 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 16 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 99 00 00
command: 17 00 00 00
#
name: AudioMode
type: parsed
protocol: NECext
address: 00 99 00 00
command: 18 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 99 00 00
command: 19 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1A 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1B 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1D 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1E 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1F 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 00 99 00 00
command: 40 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 4D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 99 00 00
command: 4E 00 00 00
#
name: O))
type: parsed
protocol: NECext
address: 00 99 00 00
command: 53 00 00 00
#
name: Camcorder
type: parsed
protocol: NECext
address: 00 99 00 00
command: 54 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 00 99 00 00
command: 55 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 00 99 00 00
command: 56 00 00 00
#
name: ||>
type: parsed
protocol: NECext
address: 00 99 00 00
command: 57 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5B 00 00 00
#
name: UpArrow
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5C 00 00 00
#
name: DownArrow
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5D 00 00 00
#
name: LeftArrow
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5E 00 00 00
#
name: RightArrow
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5F 00 00 00
