Filetype: IR signals file
Version: 1
#
name: MENU_UP_ARROW
type: parsed
protocol: NECext
address: 85 02 00 00
command: 01 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 85 02 00 00
command: 01 00 00 00
#
name: OSD_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 02 00 00 00
#
name: FRONT_PANEL_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 03 00 00 00
#
name: FP_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 03 00 00 00
#
name: FRONT_PANEL_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 04 00 00 00
#
name: FP_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 04 00 00 00
#
name: OSD_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 05 00 00 00
#
name: MENU_SELECT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 08 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 08 00 00 00
#
name: MENU_DONE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0A 00 00 00
#
name: DONE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0A 00 00 00
#
name: INPUT_TAPE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0C 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0C 00 00 00
#
name: INPUT_TUNER
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0D 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0D 00 00 00
#
name: INPUT_CD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0E 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0E 00 00 00
#
name: INPUT_AUX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0F 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 0F 00 00 00
#
name: INPUT_TV
type: parsed
protocol: NECext
address: 85 02 00 00
command: 10 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 85 02 00 00
command: 10 00 00 00
#
name: INPUT_V-DISC
type: parsed
protocol: NECext
address: 85 02 00 00
command: 11 00 00 00
#
name: V_DISC
type: parsed
protocol: NECext
address: 85 02 00 00
command: 11 00 00 00
#
name: INPUT_DVD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 12 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 12 00 00 00
#
name: INPUT_VCR
type: parsed
protocol: NECext
address: 85 02 00 00
command: 13 00 00 00
#
name: VCR_1
type: parsed
protocol: NECext
address: 85 02 00 00
command: 13 00 00 00
#
name: VOLUME_MUTE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 15 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 15 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 85 02 00 00
command: 16 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 85 02 00 00
command: 17 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 18 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 19 00 00 00
#
name: FX_UP
type: parsed
protocol: NECext
address: 85 02 00 00
command: 1A 00 00 00
#
name: FX_DOWN
type: parsed
protocol: NECext
address: 85 02 00 00
command: 1B 00 00 00
#
name: MENU_DOWN_ARROW
type: parsed
protocol: NECext
address: 85 02 00 00
command: 1D 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 85 02 00 00
command: 1D 00 00 00
#
name: FX_DOLBY
type: parsed
protocol: NECext
address: 85 02 00 00
command: 20 00 00 00
#
name: DOLBY
type: parsed
protocol: NECext
address: 85 02 00 00
command: 20 00 00 00
#
name: FX_THX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 21 00 00 00
#
name: THX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 21 00 00 00
#
name: FX_LOGIC_7
type: parsed
protocol: NECext
address: 85 02 00 00
command: 22 00 00 00
#
name: LOGIC_7
type: parsed
protocol: NECext
address: 85 02 00 00
command: 22 00 00 00
#
name: FX_DTS
type: parsed
protocol: NECext
address: 85 02 00 00
command: 23 00 00 00
#
name: DTS
type: parsed
protocol: NECext
address: 85 02 00 00
command: 23 00 00 00
#
name: FX_2-CHANNEL
type: parsed
protocol: NECext
address: 85 02 00 00
command: 24 00 00 00
#
name: 2_CH
type: parsed
protocol: NECext
address: 85 02 00 00
command: 24 00 00 00
#
name: FX_PARTY
type: parsed
protocol: NECext
address: 85 02 00 00
command: 25 00 00 00
#
name: PARTY
type: parsed
protocol: NECext
address: 85 02 00 00
command: 25 00 00 00
#
name: FX_TV_MATRIX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 26 00 00 00
#
name: TV_MATRIX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 26 00 00 00
#
name: FX_MUSIC
type: parsed
protocol: NECext
address: 85 02 00 00
command: 27 00 00 00
#
name: MUSIC
type: parsed
protocol: NECext
address: 85 02 00 00
command: 27 00 00 00
#
name: R/Z-2_+_OSD_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 42 00 00 00
#
name: R/Z-2_+_FP_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 43 00 00 00
#
name: R/Z-2_+_FP_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 44 00 00 00
#
name: MENU_STATUS
type: parsed
protocol: NECext
address: 85 02 00 00
command: 45 00 00 00
#
name: Z-2_BALANCE_RIGHT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 48 00 00 00
#
name: Z-2_BALANCE_LEFT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 4A 00 00 00
#
name: R/Z-2_INPUT_TAPE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 4C 00 00 00
#
name: R/Z-2_INPUT_TUNER
type: parsed
protocol: NECext
address: 85 02 00 00
command: 4D 00 00 00
#
name: R/Z-2_INPUT_CD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 4E 00 00 00
#
name: R/Z-2_INPUT_AUX
type: parsed
protocol: NECext
address: 85 02 00 00
command: 4F 00 00 00
#
name: R/Z-2_INPUT_TV
type: parsed
protocol: NECext
address: 85 02 00 00
command: 50 00 00 00
#
name: R/Z-2_INPUT_V-DISC
type: parsed
protocol: NECext
address: 85 02 00 00
command: 51 00 00 00
#
name: R/Z-2_INPUT_DVD
type: parsed
protocol: NECext
address: 85 02 00 00
command: 52 00 00 00
#
name: R/Z-2_INPUT_VCR
type: parsed
protocol: NECext
address: 85 02 00 00
command: 53 00 00 00
#
name: Z-2_MUTE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 55 00 00 00
#
name: Z-2_VOL-
type: parsed
protocol: NECext
address: 85 02 00 00
command: 56 00 00 00
#
name: Z-2_VOL+
type: parsed
protocol: NECext
address: 85 02 00 00
command: 57 00 00 00
#
name: Z-2_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 58 00 00 00
#
name: Z-2_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 59 00 00 00
#
name: MENU_LOCK_ON_LOCK
type: parsed
protocol: NECext
address: 85 02 00 00
command: 5A 00 00 00
#
name: R/Z-2_+_FX_DOWN
type: parsed
protocol: NECext
address: 85 02 00 00
command: 5B 00 00 00
#
name: Z-2_VOLUME_TO_-30DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 60 00 00 00
#
name: Z-2_VOLUME_TO_-20DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 61 00 00 00
#
name: Z-2_VOLUME_TO_-10DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 62 00 00 00
#
name: Z-2_VOLUME_TO_+00DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 63 00 00 00
#
name: VOLUME_TO_-30_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 64 00 00 00
#
name: VOLUME_TO_-20_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 65 00 00 00
#
name: VOLUME_TO_-10_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 66 00 00 00
#
name: VOLUME_TO_+00_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 67 00 00 00
#
name: BALANCE_FRONT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 81 00 00 00
#
name: FRONT_FADER
type: parsed
protocol: NECext
address: 85 02 00 00
command: 81 00 00 00
#
name: MENU_BACK_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 82 00 00 00
#
name: SHIFT_+_FP_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 83 00 00 00
#
name: SHIFT_+_FP_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 84 00 00 00
#
name: MENU_BACK_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 85 00 00 00
#
name: BALANCE_RIGHT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 88 00 00 00
#
name: R_BALANCE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 88 00 00 00
#
name: BALANCE_LEFT
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8A 00 00 00
#
name: L_BALANCE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8A 00 00 00
#
name: EQ_LOUDNESS_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8C 00 00 00
#
name: LOUDNESS_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8C 00 00 00
#
name: EQ_TILT_-
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8D 00 00 00
#
name: EQ_TREBLE_-
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8E 00 00 00
#
name: TREBLE_DOWN
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8E 00 00 00
#
name: EQ_BASS_-
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8F 00 00 00
#
name: BASS_LEVEL_DOWN
type: parsed
protocol: NECext
address: 85 02 00 00
command: 8F 00 00 00
#
name: EQ_LOUDNESS_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 90 00 00 00
#
name: LOUDNESS_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 90 00 00 00
#
name: EQ_TILT_+
type: parsed
protocol: NECext
address: 85 02 00 00
command: 91 00 00 00
#
name: EQ_TREBLE_+
type: parsed
protocol: NECext
address: 85 02 00 00
command: 92 00 00 00
#
name: TREBLE_UP
type: parsed
protocol: NECext
address: 85 02 00 00
command: 92 00 00 00
#
name: EQ_BASS_+
type: parsed
protocol: NECext
address: 85 02 00 00
command: 93 00 00 00
#
name: BASS_LEVEL_UP
type: parsed
protocol: NECext
address: 85 02 00 00
command: 93 00 00 00
#
name: VOLUME_FULL_MUTE
type: parsed
protocol: NECext
address: 85 02 00 00
command: 95 00 00 00
#
name: VOL-5_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 96 00 00 00
#
name: VOL+5_DB
type: parsed
protocol: NECext
address: 85 02 00 00
command: 97 00 00 00
#
name: PGM_TRIGGER_ON
type: parsed
protocol: NECext
address: 85 02 00 00
command: 98 00 00 00
#
name: PGM_TRIGGER_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 99 00 00 00
#
name: BALANCE_CENTERED
type: parsed
protocol: NECext
address: 85 02 00 00
command: 9A 00 00 00
#
name: EQ_OFF
type: parsed
protocol: NECext
address: 85 02 00 00
command: 9B 00 00 00
#
name: BALANCE_REAR
type: parsed
protocol: NECext
address: 85 02 00 00
command: 9D 00 00 00
#
name: REAR_FADER
type: parsed
protocol: NECext
address: 85 02 00 00
command: 9D 00 00 00
#
name: FX_NIGHTCLUB
type: parsed
protocol: NECext
address: 85 02 00 00
command: A0 00 00 00
#
name: NIGHTCLUB
type: parsed
protocol: NECext
address: 85 02 00 00
command: A0 00 00 00
#
name: FX_CONCERT_HALL
type: parsed
protocol: NECext
address: 85 02 00 00
command: A1 00 00 00
#
name: CONCERT_HALL
type: parsed
protocol: NECext
address: 85 02 00 00
command: A1 00 00 00
#
name: FX_CHURCH
type: parsed
protocol: NECext
address: 85 02 00 00
command: A2 00 00 00
#
name: CHURCH
type: parsed
protocol: NECext
address: 85 02 00 00
command: A2 00 00 00
#
name: FX_CATHEDRAL
type: parsed
protocol: NECext
address: 85 02 00 00
command: A3 00 00 00
#
name: CATHEDRAL
type: parsed
protocol: NECext
address: 85 02 00 00
command: A3 00 00 00
#
name: INPUT_EP_/_2-CHANNEL
type: parsed
protocol: NECext
address: 85 02 00 00
command: A4 00 00 00
#
name: FX_PANORAMA
type: parsed
protocol: NECext
address: 85 02 00 00
command: A5 00 00 00
#
name: PANORAMA
type: parsed
protocol: NECext
address: 85 02 00 00
command: A5 00 00 00
#
name: FX_MONO_LOGIC
type: parsed
protocol: NECext
address: 85 02 00 00
command: A6 00 00 00
#
name: MONO_LOGIC
type: parsed
protocol: NECext
address: 85 02 00 00
command: A6 00 00 00
#
name: FX_MUSIC_SURROUND
type: parsed
protocol: NECext
address: 85 02 00 00
command: A7 00 00 00
#
name: MUSIC_LOGIC
type: parsed
protocol: NECext
address: 85 02 00 00
command: A7 00 00 00
