Filetype: IR signals file
Version: 1
# 
# FireTV 4K Max
#
name: POWER
type: parsed
protocol: NEC
address: 03 00 00 00
command: 1D 00 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 00 7F 00 00
command: 4E B1 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 03 00 00 00
command: 11 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 03 00 00 00
command: 15 00 00 00
