Filetype: IR signals file
Version: 1
#
# SUPERBOX Smart Mini HD
# Autogenerated from ircodes/SUPERBOX/Smart Mini HD.xml
#
name: POWER
type: parsed
protocol: NECext
address: 04 02 00 00
command: C5 3A 00 00
#
name: VF
type: parsed
protocol: NECext
address: 04 02 00 00
command: 5F A0 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 02 00 00
command: 87 78 00 00
#
name: WIDE
type: parsed
protocol: NECext
address: 04 02 00 00
command: 9F 60 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 04 02 00 00
command: F5 0A 00 00
#
name: FAV
type: parsed
protocol: NECext
address: 04 02 00 00
command: E5 1A 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 02 00 00
command: F7 08 00 00
#
name: CH+
type: parsed
protocol: NECext
address: 04 02 00 00
command: ED 12 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 04 02 00 00
command: C7 38 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 02 00 00
command: 1F E0 00 00
#
name: OK
type: parsed
protocol: NECext
address: 04 02 00 00
command: 2F D0 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 02 00 00
command: 0F F0 00 00
#
name: PAGE+
type: parsed
protocol: NECext
address: 04 02 00 00
command: 45 BA 00 00
#
name: CH-
type: parsed
protocol: NECext
address: 04 02 00 00
command: AF 50 00 00
#
name: PAGE-
type: parsed
protocol: NECext
address: 04 02 00 00
command: 07 F8 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 02 00 00
command: 95 6A 00 00
#
name: RECALL
type: parsed
protocol: NECext
address: 04 02 00 00
command: CD 32 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 02 00 00
command: 55 AA 00 00
#
name: NET
type: parsed
protocol: NECext
address: 04 02 00 00
command: CF 30 00 00
#
name: USB
type: parsed
protocol: NECext
address: 04 02 00 00
command: E7 18 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 04 02 00 00
command: DD 22 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 02 00 00
command: FD 02 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 02 00 00
command: 3F C0 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 02 00 00
command: BF 40 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 02 00 00
command: B7 48 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 02 00 00
command: 97 68 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 02 00 00
command: A7 58 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 02 00 00
command: 37 C8 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 02 00 00
command: 17 E8 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 02 00 00
command: 27 D8 00 00
#
name: SAT
type: parsed
protocol: NECext
address: 04 02 00 00
command: 8F 70 00 00
#
name: 0
type: parsed
protocol: NECext
address: 04 02 00 00
command: D5 2A 00 00
#
name: TV/RADIO
type: parsed
protocol: NECext
address: 04 02 00 00
command: 57 A8 00 00
#
name: PLAY-PAUSE
type: parsed
protocol: NECext
address: 04 02 00 00
command: 0D F2 00 00
#
name: STOP-GOTO
type: parsed
protocol: NECext
address: 04 02 00 00
command: 2D D2 00 00
#
name: PLAY-BMARK
type: parsed
protocol: NECext
address: 04 02 00 00
command: 6F 90 00 00
#
name: REC-AB
type: parsed
protocol: NECext
address: 04 02 00 00
command: EF 10 00 00
#
name: REW-VIDEO-TIMER
type: parsed
protocol: NECext
address: 04 02 00 00
command: 1D E2 00 00
#
name: FWD-VIDEO-F1
type: parsed
protocol: NECext
address: 04 02 00 00
command: 3D C2 00 00
#
name: PREV-VIDEO-F2
type: parsed
protocol: NECext
address: 04 02 00 00
command: DF 20 00 00
#
name: NEXT-VIDEO-F3
type: parsed
protocol: NECext
address: 04 02 00 00
command: FF 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 04 02 00 00
command: 4D B2 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 04 02 00 00
command: 6D 92 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 04 02 00 00
command: 5D A2 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 04 02 00 00
command: 7D 82 00 00
