Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 80 00 00 00
command: 00 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 02 00 00 00
#
name: SCREEN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 03 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 80 00 00 00
command: 05 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 80 00 00 00
command: 06 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 80 00 00 00
command: 07 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 80 00 00 00
command: 08 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 80 00 00 00
command: 09 00 00 00
#
name: REPLY
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0B 00 00 00
#
name: BRIGHTNESSDOWN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0C 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 80 00 00 00
command: 10 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 11 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 12 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 13 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 14 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 80 00 00 00
command: 15 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 16 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 17 00 00 00
#
name: HOMEPAGE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1B 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1C 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1D 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1E 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1F 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 80 00 00 00
command: 40 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 80 00 00 00
command: 41 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 80 00 00 00
command: 42 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 43 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 80 00 00 00
command: 44 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 80 00 00 00
command: 45 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 80 00 00 00
command: 46 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 80 00 00 00
command: 47 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 48 00 00 00
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 49 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 80 00 00 00
command: 4A 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 80 00 00 00
command: 4D 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 80 00 00 00
command: 4E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 56 00 00 00
#
name: REDO
type: parsed
protocol: NECext
address: 80 00 00 00
command: 57 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 80 00 00 00
command: 58 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 59 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 80 00 00 00
command: 5A 00 00 00
#
name: MEDIA
type: parsed
protocol: NECext
address: 80 00 00 00
command: 5C 00 00 00
