Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 30 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 30 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 30 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 30 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 30 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 30 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 30 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 30 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 30 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 30 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 30 00 00 00
command: 0C 00 00 00
#
name: SYSTEM
type: parsed
protocol: NECext
address: 30 00 00 00
command: 0F 00 00 00
#
name: DIM
type: parsed
protocol: NECext
address: 30 00 00 00
command: 13 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 30 00 00 00
command: 1D 00 00 00
#
name: PROGPLUS
type: parsed
protocol: NECext
address: 30 00 00 00
command: 1E 00 00 00
#
name: PROGMINUS
type: parsed
protocol: NECext
address: 30 00 00 00
command: 1F 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 30 00 00 00
command: 20 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 30 00 00 00
command: 21 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 30 00 00 00
command: 22 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 30 00 00 00
command: 28 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 30 00 00 00
command: 29 00 00 00
#
name: SCAN
type: parsed
protocol: NECext
address: 30 00 00 00
command: 2A 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 30 00 00 00
command: 2C 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 30 00 00 00
command: 30 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 30 00 00 00
command: 31 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 30 00 00 00
command: 37 00 00 00
#
name: REPEATAB
type: parsed
protocol: NECext
address: 30 00 00 00
command: 3B 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 30 00 00 00
command: 41 00 00 00
#
name: TVDVD
type: parsed
protocol: NECext
address: 30 00 00 00
command: 43 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 30 00 00 00
command: 4B 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 30 00 00 00
command: 4E 00 00 00
#
name: DISC
type: parsed
protocol: NECext
address: 30 00 00 00
command: 54 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 30 00 00 00
command: 58 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 30 00 00 00
command: 59 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 30 00 00 00
command: 5A 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 30 00 00 00
command: 5B 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 30 00 00 00
command: 85 00 00 00
#
name: TC
type: parsed
protocol: NECext
address: 30 00 00 00
command: C8 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: 30 00 00 00
command: CF 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 30 00 00 00
command: EE 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 30 00 00 00
command: F7 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 30 00 00 00
command: FA 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 30 00 00 00
command: FE 00 00 00
