Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
# 
name: Home
type: parsed
protocol: NEC
address: 04 00 00 00
command: 7C 00 00 00
# 
name: Settings
type: parsed
protocol: NEC
address: 04 00 00 00
command: 43 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
# 
name: Enter
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
#
name: Back
type: parsed
protocol: NEC
address: 04 00 00 00
command: 28 00 00 00
#
name: Guide
type: parsed
protocol: NEC
address: 04 00 00 00
command: AB 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
#
name: Netflix
type: parsed
protocol: NEC
address: 04 00 00 00
command: 56 00 00 00
# 
name: Prime_video
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5C 00 00 00
# 
name: Movies
type: parsed
protocol: NEC
address: 04 00 00 00
command: 81 00 00 00
#
name: Red
type: parsed
protocol: NEC
address: 04 00 00 00
command: 72 00 00 00
# 
name: Green
type: parsed
protocol: NEC
address: 04 00 00 00
command: 71 00 00 00
# 
name: Yellow
type: parsed
protocol: NEC
address: 04 00 00 00
command: 63 00 00 00
# 
name: Blue
type: parsed
protocol: NEC
address: 04 00 00 00
command: 61 00 00 00
# 
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: B0 00 00 00
# 
name: Resume
type: parsed
protocol: NEC
address: 04 00 00 00
command: BA 00 00 00
