Filetype: IR signals file
Version: 1
# 
name: Power
type: parsed
protocol: NEC
address: 7E 00 00 00
command: 2A 00 00 00
# 
name: BD_DVD
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 00 7F 00 00
# 
name: TV
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 03 7C 00 00
# 
name: NET
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 06 79 00 00
# 
name: Radio
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 09 76 00 00
# 
name: Straight
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 56 00 00 00
# 
name: Direct
type: parsed
protocol: NEC
address: 7A 00 00 00
command: DD 00 00 00
# 
name: Enchancer
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 94 00 00 00
# 
name: Bass
type: parsed
protocol: NECext
address: 7A 85 00 00
command: BD C2 00 00
# 
name: Prog L
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 59 00 00 00
# 
name: Prog R
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 58 00 00 00
# 
name: FM/AM
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 16 00 00 00
# 
name: USB
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 72 0D 00 00
# 
name: Network
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 3F C0 00 00
# 
name: BT
type: parsed
protocol: NECext
address: 7A 85 00 00
command: BE C1 00 00
# 
name: Input +
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1F 60 00 00
# 
name: Input -
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 23 5C 00 00
# 
name: Vol +
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1A 00 00 00
# 
name: Vol -
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1B 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1C 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 9D 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 9C 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 9F 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 9E 00 00 00
# 
name: OK
type: parsed
protocol: NEC
address: 7A 00 00 00
command: DE 00 00 00
# 
name: Setup
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 84 00 00 00
# 
name: Option
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 6B 14 00 00
# 
name: Display
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 60 9F 00 00
# 
name: Return
type: parsed
protocol: NEC
address: 7A 00 00 00
command: AA 00 00 00
# 
name: Top Menu
type: parsed
protocol: NECext
address: 7A 85 00 00
command: A0 DF 00 00
# 
name: Home
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 66 99 00 00
# 
name: Pop-up Menu
type: parsed
protocol: NECext
address: 7A 85 00 00
command: A4 DB 00 00
# 
name: Red
type: parsed
protocol: NECext
address: 7A 85 00 00
command: C0 BF 00 00
# 
name: Green
type: parsed
protocol: NECext
address: 7A 85 00 00
command: C1 BE 00 00
# 
name: Yellow
type: parsed
protocol: NECext
address: 7A 85 00 00
command: C2 BD 00 00
# 
name: Blue
type: parsed
protocol: NECext
address: 7A 85 00 00
command: C3 BC 00 00
# 
name: Track Bck
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6C 93 00 00
# 
name: Track Fwd
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6D 92 00 00
# 
name: Rewind
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6A 95 00 00
# 
name: Forward
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6B 94 00 00
# 
name: Play
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 68 97 00 00
# 
name: Pause
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 67 98 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 69 96 00 00
# 
name: Preset L
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 5E 21 00 00
# 
name: Preset R
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 5B 24 00 00
# 
name: Sleep
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 30 00 00 00
