Filetype: IR signals file
Version: 1
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 06 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 07 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 08 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 09 00 00 00
#
name: input
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 04 00 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 00 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 00 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 00 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 00 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 00 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 00 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 00 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 00 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 00 00 00
command: 19 00 00 00
#
name: q.view
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1A 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1E 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 20 00 00 00
#
name: av-mode
type: parsed
protocol: NECext
address: 04 00 00 00
command: 30 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 40 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 41 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 00 00 00
command: 43 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 04 00 00 00
command: 44 00 00 00
#
name: q.manu
type: parsed
protocol: NECext
address: 04 00 00 00
command: 45 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 04 00 00 00
command: 53 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5B 00 00 00
#
name: pip
type: parsed
protocol: NECext
address: 04 00 00 00
command: 60 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 61 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 04 00 00 00
command: 63 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 71 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 04 00 00 00
command: 72 00 00 00
#
name: xstudio
type: parsed
protocol: NECext
address: 04 00 00 00
command: 7C 00 00 00
#
name: simplink
type: parsed
protocol: NECext
address: 04 00 00 00
command: 7E 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 04 00 00 00
command: 8E 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 04 00 00 00
command: 8F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 04 00 00 00
command: B0 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 04 00 00 00
command: B1 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 04 00 00 00
command: BA 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 04 00 00 00
command: BD 00 00 00
