Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: A6 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A6 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A6 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A6 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A6 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A6 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A6 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A6 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A6 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: A6 00 00 00
command: 09 00 00 00
#
name: VOLRIGHT
type: parsed
protocol: NECext
address: A6 00 00 00
command: 0A 00 00 00
#
name: VOLLEFT
type: parsed
protocol: NECext
address: A6 00 00 00
command: 0B 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: A6 00 00 00
command: 1E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: A6 00 00 00
command: 42 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A6 00 00 00
command: 43 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A6 00 00 00
command: 44 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: A6 00 00 00
command: 45 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: A6 00 00 00
command: 46 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: A6 00 00 00
command: 4A 00 00 00
#
name: CHDWN
type: parsed
protocol: NECext
address: A6 00 00 00
command: 4B 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: A6 00 00 00
command: 4F 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: A6 00 00 00
command: 52 00 00 00
#
name: ENT
type: parsed
protocol: NECext
address: A6 00 00 00
command: FF 00 00 00
